Speaker

1. 기  능

본 기기는 8인치로 구성된 2way 스피커로서, 높은 명료도와 자연스러운 사운드를 얻을 수 있어야 한다. 18mm 합판과 인클로저로 되어 깨끗한 보컬 주파수 특성, 낮은 레벨에서 높은 레벨까지 왜곡이 없고, 음질 변화 없이 재생할 수 있어야 한다. 생음악, 음악 재생 및 연설을 포함하여 다양한 공간에서 적절하다.

2. 사  양

- Frequency Response(1W@1m)

±3dB	: 90Hz~20KHz

-10dB	: 80Hz~22KHz

- Axial Sensitivity(dB SPL,1W@1m): 96

- Impedance(Ohms)	: 8

- Power Handling RMS/PROGRAM/PEAK(Watts) : 175/350/700

- Calculated Maximum Output(dB SPL@1m)

Full Range peak	: 110

Full Range Long Term	: 105

- Nominal Coverage Angle/-6dB points(Degrees)

Horizontal	: 90

Vertical	: 90

- System configuration	: Two-way full range

- Powering	: Passive(LF/HF crossover)

- LF subsystem	: 8" Woofer ×1

- HF subsystem	: 1"HF system protection circuit/Ferrofluid oil coolant

- Enclosure Materials	: High intensity 15mm wood

- Finish/color	: Water resistant textured/Black or White

- Connectors	: NL4 Speakon×2

- Hardware

Top/Bottom	: Suspend Point×2

Rear	: Suspend Point×1

Right/Left	: Suspend Point×2

- Grille	: Power coated perforated steel, foam backed

- Weight

Net.	: 8.2kg

Gross	: 9.5kg

- Dimensions(W×H×D)	: 9.7"×17.5"×9.3"(247mm×445mm×236mm)

◎ MSR0810 및 동등 이상품